|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | アイスクリームフリーザー (Electric ice cream freezers) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 電動機の定格消費電力 (Rated input of electric motor) | [ ]  (1) 30Ｗ以下のもの (30W or less)[ ]  (2) 30Ｗを超え40Ｗ以下のもの (Exceeding 30W, and less than or equal to 40W)[ ]  (3) 40Ｗを超え50Ｗ以下のもの (Exceeding 40W, and less than or equal to 50W)[ ]  (4) 50Ｗを超え60Ｗ以下のもの (Exceeding 50W, and less than or equal to 60W)[ ]  (5) 60Ｗを超え70Ｗ以下のもの (Exceeding 60W, and less than or equal to 70W)[ ]  (6) 70Ｗを超え80Ｗ以下のもの (Exceeding 70W, and less than or equal to 80W)[ ]  (7) 80Ｗを超え90Ｗ以下のもの (Exceeding 80W, and less than or equal to 90W)[ ]  (8) 90Ｗを超え100Ｗ以下のもの (Exceeding 90W, and less than or equal to 100W)[ ]  (9) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)[ ]  (10) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)[ ]  (11) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)[ ]  (12) 400Ｗを超え500Ｗ以下のもの (Exceeding 400W, and less than or equal to 500W)[ ]  (13) 500Ｗを超えるもの (Exceeding 500W) |
|  | 容器と本体との分離 (Container and body) | [ ]  (1) できるもの (Detachable)[ ]  (2) できないもの (Non-detachable) |
|  | 定格周波数 (Rated frequency) | [ ]  (1) 50Hzのもの (50Hz)[ ]  (2) 60Hzのもの (60Hz) |
|  | 定格時間 (Rated time) | [ ]  (1) 30分以下の短時間定格のもの (Short time rated, thirty minutes or less)[ ]  (2) 30分を超える短時間定格のもの (Short time rated, exceeding thirty minutes)[ ]  (3) 連続定格のもの (Continuous rated) |
|  | 冷却装置 (Cooling device) | [ ]  (1) あるもの (With cooling device)[ ]  (2) ないもの (Without cooling device) |
|  | 電動機の種類 (Type of motor) | [ ]  (1) 分相始動誘導電動機のもの (Split phase starting induction motor)[ ]  (2) コンデンサー始動誘導電動機のもの (Capacity-start induction motor)[ ]  (3) コンデンサー誘導電動機のもの (Capacity-run induction motor)[ ]  (4) くま取りコイル誘導電動機のもの (Shaded-pole induction motor)[ ]  (5) 整流子電動機のもの (Commutator motor)[ ]  (6) その他のもの (Others) |
|  | 電動機の極 (Number of motor poles) | [ ]  (1) ２極のもの (Two poles)[ ]  (2) ４極のものFour poles)[ ]  (3) ６極のもの (Six poles)[ ]  (4) ８極以上のもの (Eight or more poles) |
|  | 電動機の巻線の絶縁の種類 (Motor winding insulation class) | [ ]  (1) Ａ種のもの (Class A)[ ]  (2) Ｅ種のもの (Class E)[ ]  (3) Ｂ種のもの (Class B)[ ]  (4) Ｆ種のもの (Class F)[ ]  (5) Ｈ種のもの (Class H)[ ]  (6) その他のもの (Others) |
|  | 電熱装置 (Electric heating device) | [ ]  (1) あるもの (With heating device)[ ]  (2) ないもの (Without heating device) |
|  | 電熱装置の定格消費電力 (Rated input of electric heating device) | [ ]  (1) 100Ｗ以下のもの (100W or less)[ ]  (2) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)[ ]  (3) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)[ ]  (4) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)[ ]  (5) 400Ｗを超え500Ｗ以下のもの (Exceeding 400W, and less than or equal to 500W)[ ]  (6) 500Ｗを超え600Ｗ以下のもの (Exceeding 500W, and less than or equal to 600W)[ ]  (7) 600Ｗを超え700Ｗ以下のもの (Exceeding 600W, and less than or equal to 700W)[ ]  (8) 700Ｗを超え800Ｗ以下のもの (Exceeding 700W, and less than or equal to 800W)[ ]  (9) 800Ｗを超え900Ｗ以下のもの (Exceeding 800W, and less than or equal to 900W)[ ]  (10) 900Ｗを超えるもの (Exceeding 900W) |
|  | 自動スイッチ（温度過昇防止装置として用いられるものを除く。） (Temperature limiter (excluding those used for thermal cutout.)) | [ ]  (1) あるもの (With temperature limiter)[ ]  (2) ないもの (Without temperature limiter) |
|  | 自動スイッチの動作温度の設定 (Temperature limiter operating temperature setting) | [ ]  (1) 固定しているもの (Fixed)[ ]  (2) 可変のもの (Adjustable) |
|  | 自動スイッチの動作温度（動作温度が可変のものにあつては、その最高の温度をいう。） (Temperature limiter operating temperature (in the case of switches with adjustable operating temperature, the maximum temperature.)) | [ ]  (1) 80℃以下のもの (80℃ or less)[ ]  (2) 80℃を超え100℃以下のもの (Exceeding 80℃, and less than or equal to 100℃)[ ]  (3) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)[ ]  (4) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)[ ]  (5) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)[ ]  (6) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)[ ]  (7) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)[ ]  (8) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)[ ]  (9) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)[ ]  (10) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)[ ]  (11) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)[ ]  (12) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)[ ]  (13) 300℃を超えるもの (Exceeding 300℃) |
|  | 器体スイッチ（主回路を開閉するものの場合に限り、自動スイッチ及び自動温度調節器を除く。） (Body switch (limited to those used for turning the main circuit on and off, and excluding temperature limiters and thermostats.)) | [ ]  (1) あるもの (With body switch)[ ]  (2) ないもの (Without body switch) |
|  | 器体スイッチの操作の方式 (Switching operation of body switch) | [ ]  (1) タンブラー式のもの (Tumbler type)[ ]  (2) 押しボタン式のもの (Push button type)[ ]  (3) ロータリー式のもの (Rotary type)[ ]  (4) 引きひも式のもの (Pull cord type)[ ]  (5) 電磁式のもの (Electromagnetic type)[ ]  (6) その他のもの (Others) |
|  | 器体スイッチの接点の材料 (Body switch contact materials) | [ ]  (1) 銀のもの又は銀合金のもの (Silver or silver alloy)[ ]  (2) 銅のもの又は銅合金のもの (Copper or copper alloy)[ ]  (3) その他のもの (Others) |
|  | 変圧器 (Transformer) | [ ]  (1) あるもの (With transformer)[ ]  (2) ないもの (Without transformer) |
|  | 変圧器の巻線の絶縁の種類 (Transformer winding insulation class) | [ ]  (1) Ａ種のもの (Class A)[ ]  (2) Ｅ種のもの (Class E)[ ]  (3) Ｂ種のもの (Class B)[ ]  (4) Ｆ種のもの (Class F)[ ]  (5) Ｈ種のもの (Class H)[ ]  (6) その他のもの (Others) |
|  | 種類 (Type) | [ ]  (1) 手持ち型のもの (Handheld type)[ ]  (2) 卓上型又は床上型のもの (Tabletop type or floor type)[ ]  (3) その他のもの (Others) |
|  | 電源電線と器体との接続の方式 (Power supply connections) | [ ]  (1) 直付けのもの (Fixed to the appliance)[ ]  (2) 接続器利用のもの (Coupling device) |
|  | 電線巻取機構 (Cord reel) | [ ]  (1) あるもの (With cord reel)[ ]  (2) ないもの (Without cord reel) |
|  | 二重絶縁 (Double insulation) | [ ]  (1) 施してあるもの (With double insulation)[ ]  (2) 施してないもの (Without double insulation) |