|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | 箱開閉器 (Box switches) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 定格電流（定格電流表示のあるものの場合に限る。） (Rated current (limited to those with rated current markings.)) | [ ]  (1) ５Ａ以下のもの (7A or less)[ ]  (2) ５Ａを超え15Ａ以下のもの (Exceeding 5A, and less than or equal to 15A)[ ]  (3) 15Ａを超え30Ａ以下のもの (Exceeding 15A, and less than or equal to 30A)[ ]  (4) 30Ａを超え60Ａ以下のもの (Exceeding 30A, and less than or equal to 60A)[ ]  (5) 60Ａを超えるもの (Exceeding 60A) |
|  | 適用電動機の定格容量（適用電動機の定格容量表示のあるものの場合に限る。） (Rated capacity of applicable motor (limited to those with rated current markings for applicable motors.)) | [ ]  (1) 単相で200Ｗ以下のもの (Single phase, 200W or less)[ ]  (2) 単相で200Ｗを超え400Ｗ以下のもの (Single phase, exceeding 200W, and less than or equal to 400W)[ ]  (3) 単相で400Ｗを超え750Ｗ以下のもの (Single phase, exceeding 400W, and less than or equal to 750W)[ ]  (4) 単相で750Ｗを超えるもの (Single phase, exceeding 750W)[ ]  (5) ３相で750Ｗ以下のもの (Three phase, 750W or less)[ ]  (6) ３相で750Ｗを超え2.2kW以下のもの (Three phase, Exceeding 750W, and less than or equal to 2.2kW)[ ]  (7) ３相で2.2kWを超え3.7kW以下のもの (Three phase, Exceeding 2.2kW, and less than or equal to 3.7kW)[ ]  (8) ３相で3.7kWを超え7.5kW以下のもの (Three phase, Exceeding 3.7kW, and less than or equal to 7.5kW)[ ]  (9) ３相で7.5kWを超えるもの (Three phase, Exceeding 7.5kW) |
|  | 極 (Poles) | [ ]  (1) ２極以下のもの (Two poles or less)[ ]  (2) ３極以上のもの (Three or more poles) |
|  | 電源側接続端子 (Power supply terminals) | [ ]  (1) ねじ端子のもの (Cord connected type)[ ]  (2) プラグイン式のもの (Plug-in type)[ ]  (3) その他のもの (Others) |
|  | 接続する電線の種類 (Type of cable or cord to which switch is connected) | [ ]  (1) 銅のもの (Copper)[ ]  (2) その他のもの (Others) |
|  | ヒューズの取付け部 (Fuse holder) | [ ]  (1) あるもの (With fuse holder)[ ]  (2) ないもの (Without fuse holder) |
|  | 取付けヒューズの種類 (Type of attached fuse) | [ ]  (1) つめ付ヒューズのもの (Link fuse)[ ]  (2) 筒形ヒューズのもの (Tubular fuse)[ ]  (3) 栓形ヒューズのもの (Plug fuse)[ ]  (4) その他のもの (Others) |
|  | 開閉接触部の構造 (Construction of switching contacts) | [ ]  (1) 刃形のもの (Knife blade shape)[ ]  (2) 塊状のもの (Solid shape)[ ]  (3) その他のもの (Others) |
|  | 接点の材料 (Contact materials) | [ ]  (1) 銀のもの又は銀合金のもの (Silver or silver alloy)[ ]  (2) 銅のもの又は銅合金のもの (Copper or copper alloy)[ ]  (3) その他のもの (Others) |
|  | 過電流引き外し素子 (Over current tripping elements) | [ ]  (1) あるもの (With over current tripping elements)[ ]  (2) ないもの (Without over current tripping elements) |
|  | 過電流引き外し素子の数 (Number of over current tripping elements) | [ ]  (1) １のもの (One)[ ]  (2) ２のもの (Two)[ ]  (3) ３以上のもの (Three or more) |
|  | 過電流引き外し機構 (Over current tripping mechanism) | [ ]  (1) 熱動式のもの (Thermal type)[ ]  (2) 電磁式のもの (Electromagnetic type)[ ]  (3) その他のもの (Others) |
|  | 外郭の材料 (Outer case materials) | [ ]  (1) 金属のもの (Metal)[ ]  (2) 合成樹脂のもの (Plastic)[ ]  (3) その他のもの (Others) |
|  | 定格遮断電流（定格遮断電流表示のあるものの場合に限る。） (Rated breaking capacity (limited to those with breaking capacity markings.)) | [ ]  (1) 1,000Ａ以下のもの (1,000A or less)[ ]  (2) 1,000Ａを超え1,500Ａ以下のもの (Exceeding 1,000A, and less than or equal to 1,500A)[ ]  (3) 1,500Ａを超え2,500Ａ以下のもの (Exceeding 1,500A, and less than or equal to 2,500A)[ ]  (4) 2,500Ａを超え5,000Ａ以下のもの (Exceeding 2,500A, and less than or equal to 5,000A)[ ]  (5) 5,000Ａを超え7,500Ａ以下のもの (Exceeding 5,000A, and less than or equal to 7,500A)[ ]  (6) 7,500Ａを超え10,000Ａ以下のもの (Exceeding 7,500A, and less than or equal to 10,000A)[ ]  (7) 10,000Ａを超え15,000Ａ以下のもの (Exceeding 10,000A, and less than or equal to 15,000A)[ ]  (8) 15,000Ａを超え20,000Ａ以下のもの (Exceeding 15,000A, and less than or equal to 20,000A)[ ]  (9) 20,000Ａを超え25,000Ａ以下のもの (Exceeding 20,000A, and less than or equal to 25,000A)[ ]  (10) 25,000Ａを超え30,000Ａ以下のもの (Exceeding 25,000A, and less than or equal to 30,000A)[ ]  (11) 30,000Ａを超えるもの (Exceeding 30,000A) |
|  | 定格コード保護電流（定格コード保護電流表示のあるものの場合に限る。） (Rated cord protection current (limited to those with rated cord protection current markings.)) | [ ]  (1) 1,000Ａ以下のもの (1,000A or less)[ ]  (2) 1,000Ａを超え1,500Ａ以下のもの (Exceeding 1,000A, and less than or equal to 1,500A)[ ]  (3) 1,500Ａを超え2,500Ａ以下のもの (Exceeding 1,500A, and less than or equal to 2,500A)[ ]  (4) 2,500Ａを超え5,000Ａ以下のもの (Exceeding 2,500A, and less than or equal to 5,000A)[ ]  (5) 5,000Ａを超えるもの (Exceeding 5,000A) |
|  | 防水構造 (Type of waterproof) | [ ]  (1) 防雨型のもの (Rainproof type)[ ]  (2) 防浸型のもの (Immersion proof type)[ ]  (3) 非防水型のもの (Non-waterproof type) |