|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | 定額制用電流制限器 (Flat rate current limiters) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 相及び線式 (Phase and wiring type) | [ ]  (1) 単相２線式のもの (Single phase, two wire type)[ ]  (2) 単相３線式のもの (Single phase, three wire type)[ ]  (3) その他のもの (Others) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 定格電流 (Rated current) | [ ]  (1) ５Ａ以下のもの (5A or less)[ ]  (2) ５Ａを超え7.5Ａ以下のもの (Exceeding 5A, and less than or equal to 7.5A)[ ]  (3) 7.5Ａを超え10Ａ以下のもの (Exceeding 7.5A, and less than or equal to 10A)[ ]  (4) 10Ａを超え15Ａ以下のもの (Exceeding 10A, and less than or equal to 15A)[ ]  (5) 15Ａを超え20Ａ以下のもの (Exceeding 15A, and less than or equal to 20A)[ ]  (6) 20Ａを超え25Ａ以下のもの (Exceeding 20A, and less than or equal to 25A)[ ]  (7) 25Ａを超え30Ａ以下のもの (Exceeding 25A, and less than or equal to 30A)[ ]  (8) 30Ａを超え40Ａ以下のもの (Exceeding 30A, and less than or equal to 40A)[ ]  (9) 40Ａを超え50Ａ以下のもの (Exceeding 40A, and less than or equal to 50A)[ ]  (10) 50Ａを超え60Ａ以下のもの (Exceeding 50A, and less than or equal to 60A)[ ]  (11) 60Ａを超えるもの (Exceeding 60A) |
|  | 極 (Poles) | [ ]  (1) 単極のもの (Single poles)[ ]  (2) ２極のもの (Two poles)[ ]  (3) ３極以上のもの (Three or more poles) |
|  | 接続する電線の種類 (Type of cable or cord to be connected) | [ ]  (1) 銅のもの (Copper)[ ]  (2) その他のもの (Others) |
|  | 過電流引き外し素子の数 (Number of over current tripping elements) | [ ]  (1) １のもの (One)[ ]  (2) ２以上のもの (Two or more) |
|  | 過電流引き外し機構 (Overcurrent tripping mechanism) | [ ]  (1) 熱動式のもの (Thermal type)[ ]  (2) 電磁式のもの (Electromagnetic type)[ ]  (3) その他のもの (Others) |
|  | 接点の材料 (Contact materials) | [ ]  (1) 銀のもの又は銀合金のもの (Silver or silver alloy)[ ]  (2) 銅のもの又は銅合金のもの (Copper or copper alloy)[ ]  (3) その他のもの (Others) |
|  | 開閉操作の方式 (Switching operation) | [ ]  (1) タンブラー式のもの (Tumbler type)[ ]  (2) 押しボタン式のもの (Push button type)[ ]  (3) 引きひも式のもの (Pull cord type)[ ]  (4) その他のもの (Others) |
|  | 外郭の材料 (Outer case materials) | [ ]  (1) 金属のもの (Metal)[ ]  (2) 合成樹脂のもの (Plastic)[ ]  (3) その他のもの (Others) |
|  | 使用場所 (Place for use) | [ ]  (1) 屋外のもの (Outdoors)[ ]  (2) 屋内のもの (Indoors) |
|  | 定格遮断電流 (Rated breaking capacity) | [ ]  (1) 1,000Ａ以下のもの (1,000A or less)[ ]  (2) 1,000Ａを超え1,500Ａ以下のもの (Exceeding 1,000A, and less than or equal to 1,500A)[ ]  (3) 1,500Ａを超え2,500Ａ以下のもの (Exceeding 1,500A, and less than or equal to 2,500A)[ ]  (4) 2,500Ａを超え5,000Ａ以下のもの (Exceeding 2,500A, and less than or equal to 5,000A)[ ]  (5) 5,000Ａを超え7,500Ａ以下のもの (Exceeding 5,000A, and less than or equal to 7,500A)[ ]  (6) 7,500Ａを超え10,000Ａ以下のもの (Exceeding 7,500A, and less than or equal to 10,000A)[ ]  (7) 10,000Ａを超え15,000Ａ以下のもの (Exceeding 10,000A, and less than or equal to 15,000A)[ ]  (8) 15,000Ａを超え20,000Ａ以下のもの (Exceeding 15,000A, and less than or equal to 20,000A)[ ]  (9) 20,000Ａを超え25,000Ａ以下のもの (Exceeding 20,000A, and less than or equal to 25,000A)[ ]  (10) 25,000Ａを超え30,000Ａ以下のもの (Exceeding 25,000A, and less than or equal to 30,000A)[ ]  (11) 30,000Ａを超えるもの (Exceeding 30,000A) |