|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | スチームバス用電熱器 (Electric heaters for steam baths) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 相 (Phase) | [ ]  (1) 単相のもの (Single phase)[ ]  (2) ３相のもの (Three phase) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 定格電流（電極式のものの場合に限る。） (Rated current (limited to electrode type.)) | [ ]  (1) １Ａ以下のもの (1A or less)[ ]  (2) １Ａを超え５Ａ以下のもの (Exceeding 1A, and less than or equal to 5A)[ ]  (3) ５Ａを超え10Ａ以下のもの (Exceeding 5A, and less than or equal to 10A)[ ]  (4) 10Ａを超え20Ａ以下のもの (Exceeding 10A, and less than or equal to 20A)[ ]  (5) 20Ａを超え30Ａ以下のもの (Exceeding 20A, and less than or equal to 30A)[ ]  (6) 30Ａを超え50Ａ以下のもの (Exceeding 30A, and less than or equal to 50A)[ ]  (7) 50Ａを超え70Ａ以下のもの (Exceeding 50A, and less than or equal to 70A)[ ]  (8) 70Ａを超えるもの (Exceeding 70A) |
|  | 定格消費電力（電極式のもの以外のものの場合に限る。） (Rated Input (limited to appliances other than electrode type.)) | [ ]  (1) 10Ｗ以下のもの (10W or less)[ ]  (2) 10Ｗを超え20Ｗ以下のもの (Exceeding 10W, and less than or equal to 20W)[ ]  (3) 20Ｗを超え30Ｗ以下のもの (Exceeding 20W, and less than or equal to 30W)[ ]  (4) 30Ｗを超え40Ｗ以下のもの (Exceeding 30W, and less than or equal to 40W)[ ]  (5) 40Ｗを超え50Ｗ以下のもの (Exceeding 40W, and less than or equal to 50W)[ ]  (6) 50Ｗを超え60Ｗ以下のもの (Exceeding 50W, and less than or equal to 60W)[ ]  (7) 60Ｗを超え70Ｗ以下のもの (Exceeding 60W, and less than or equal to 70W)[ ]  (8) 70Ｗを超え80Ｗ以下のもの (Exceeding 70W, and less than or equal to 80W)[ ]  (9) 80Ｗを超え90Ｗ以下のもの (Exceeding 80W, and less than or equal to 90W)[ ]  (10) 90Ｗを超え100Ｗ以下のもの (Exceeding 90W, and less than or equal to 100W)[ ]  (11) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)[ ]  (12) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)[ ]  (13) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)[ ]  (14) 400Ｗを超え500Ｗ以下のもの (Exceeding 400W, and less than or equal to 500W)[ ]  (15) 500Ｗを超え600Ｗ以下のもの (Exceeding 500W, and less than or equal to 600W)[ ]  (16) 600Ｗを超え700Ｗ以下のもの (Exceeding 600W, and less than or equal to 700W)[ ]  (17) 700Ｗを超え800Ｗ以下のもの (Exceeding 700W, and less than or equal to 800W)[ ]  (18) 800Ｗを超え900Ｗ以下のもの (Exceeding 800W, and less than or equal to 900W)[ ]  (19) 900Ｗを超え１kW以下のもの (Exceeding 900W, and less than or equal to 1kW)[ ]  (20) １kWを超え２kW以下のもの (Exceeding 1kW, and less than or equal to 2kW)[ ]  (21) ２kWを超え３kW以下のもの (Exceeding 2kW, and less than or equal to 3kW)[ ]  (22) ３kWを超え５kW以下のもの (Exceeding 3kW, and less than or equal to 5kW)[ ]  (23) ５kWを超え７kW以下のもの (Exceeding 5kW, and less than or equal to 7kW)[ ]  (24) ７kWを超えるもの (Exceeding 7kW) |
|  | 定格周波数（電動機又は変圧器を有するものの場合に限る。） (Rated frequency (limited to those with motors or transformers.)) | [ ]  (1) 50Hzのもの (50Hz)[ ]  (2) 60Hzのもの (60Hz) |
|  | 器体スイッチ（主回路を開閉するものの場合に限り、自動スイッチ及び自動温度調節器を除く。） (Body switch (limited to those used for turning the main circuit on and off, and excluding temperature limiters and thermostats.)) | [ ]  (1) あるもの (With body switch)[ ]  (2) ないもの (Without body switch) |
|  | 器体スイッチの操作の方式 (Switching operation of body switch) | [ ]  (1) タンブラー式のもの (Tumbler type)[ ]  (2) 押しボタン式のもの (Push button type)[ ]  (3) ロータリー式のもの (Rotary type)[ ]  (4) 電磁式のもの (Electromagnetic type)[ ]  (5) その他のもの (Others) |
|  | 器体スイッチの接点の材料 (Body switch contact material) | [ ]  (1) 銀のもの又は銀合金のもの (Silver or silver alloy)[ ]  (2) 銅のもの又は銅合金のもの (Copper or copper alloy)[ ]  (3) その他のもの (Others) |
|  | 自動スイッチ（温度過昇防止装置として用いられるものを除く。） (Temperature limiter (excluding those used for thermal cutout.)) | [ ]  (1) あるもの (With temperature limiter)[ ]  (2) ないもの (Without temperature limiter) |
|  | 自動スイッチの動作温度の設定 (Temperature limiter operating temperature setting) | [ ]  (1) 固定しているもの (Fixed)[ ]  (2) 可変のもの (Adjustable) |
|  | 自動スイッチの動作温度（動作温度が可変のものにあつては、その最高の温度をいう。） (Temperature limiter operating temperature (in the case of switches with adjustable operating temperature, the maximum temperature.)) | [ ]  (1) 80℃以下のもの (80℃ or less)[ ]  (2) 80℃を超え100℃以下のもの (Exceeding 80℃, and less than or equal to 100℃)[ ]  (3) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)[ ]  (4) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)[ ]  (5) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)[ ]  (6) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)[ ]  (7) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)[ ]  (8) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)[ ]  (9) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)[ ]  (10) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)[ ]  (11) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)[ ]  (12) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)[ ]  (13) 300℃を超えるもの (Exceeding 300℃) |
|  | 自動温度調節器（温度過昇防止装置として用いられるものを除き、電熱装置から発生する熱により動作するものに限る。） (Thermostat (excluding those used for thermal cutout, and limited to those operating from the heat generated from the electrical heating appliance.)) | [ ]  (1) あるもの (With thermostat)[ ]  (2) ないもの (Without thermostat) |
|  | 自動温度調節器の温度検知の方式 (Thermostat temperature detection method) | [ ]  (1) バイメタル式のもの (Bimetal type)[ ]  (2) 液体膨張式のもの (Liquid expansion type)[ ]  (3) 気体膨張式のもの (Gas expansion type)[ ]  (4) 半導体式のもの (Semiconductor type)[ ]  (5) その他のもの (Others) |
|  | 自動温度調節器の温度調節の方式 (Thermostat temperature setting method) | [ ]  (1) 接点を機械的に開閉するもの (Mechanical contacts)[ ]  (2) その他のもの (Others) |
|  | 自動温度調節器の動作温度（接点を機械的に開閉するものの場合に限り、かつ、動作温度が可変のものにあつては、その最高温度をいう。） (Thermostat operating temperature (limited to those using mechanical opening and closing of contacts, and, in the case of those with adjustable operating temperature, the maximum temperature.)) | [ ]  (1) 80℃以下のもの (80℃ or less)[ ]  (2) 80℃を超え100℃以下のもの (Exceeding 80℃, and less than or equal to 100℃)[ ]  (3) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)[ ]  (4) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)[ ]  (5) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)[ ]  (6) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)[ ]  (7) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)[ ]  (8) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)[ ]  (9) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)[ ]  (10) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)[ ]  (11) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)[ ]  (12) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)[ ]  (13) 300℃を超えるもの (Exceeding 300℃) |
|  | 発熱部の形態 (Type of heat generating component) | [ ]  (1) ボビン式のもの (Bobbin type)[ ]  (2) 熱板式のもの (Heating plate type)[ ]  (3) シーズ式（鋳込み式を含む。）のもの (Sheath type (including cast type.))[ ]  (4) リボン式のもの (Ribbon type)[ ]  (5) マイカ式のもの (Mica type)[ ]  (6) スペース式のもの (Space type)[ ]  (7) ドータイト式のもの (Dohtaito type)[ ]  (8) 石英管式のもの (Quartz tube type)[ ]  (9) 被覆式のもの (Covered type)[ ]  (10) ランプ式のもの (Lamp type)[ ]  (11) 半導体利用のもの (Semiconductor type)[ ]  (12) 電極式のもの (Electrode type)[ ]  (13) その他のもの (Others) |
|  | 電源電線と器体との接続の方式 (Power supply connections) | [ ]  (1) 直付けのもの (Fixed to the appliance)[ ]  (2) 接続器利用のもの (Coupling device) |
|  | 附属電動機 (Motor) | [ ]  (1) あるもの (With motor)[ ]  (2) ないもの (Without motor) |
|  | 附属電動機の種類 (Type of motor) | [ ]  (1) 誘導電動機のもの (Induction motor)[ ]  (2) 整流子電動機のもの (Commutator motor)[ ]  (3) その他のもの (Others) |
|  | 附属電動機の巻線の絶縁の種類 (Motor winding insulation class) | [ ]  (1) Ａ種のもの (Class A)[ ]  (2) Ｅ種のもの (Class E)[ ]  (3) Ｂ種のもの (Class B)[ ]  (4) Ｆ種のもの (Class F)[ ]  (5) Ｈ種のもの (Class H)[ ]  (6) その他のもの (Others) |
|  | 温度過昇防止装置 (Thermal cutout) | [ ]  (1) あるもの (With thermal cutout)[ ]  (2) ないもの (Without thermal cutout) |
|  | 温度過昇防止装置の種類 (Type of thermal cutout) | [ ]  (1) バイメタル式のもの (Bimetal type)[ ]  (2) 温度ヒューズ式のもの (Thermal link type)[ ]  (3) その他のもの (Others) |
|  | 温度過昇防止装置の動作温度 (Operating temperature of thermal cutout) | [ ]  (1) 100℃以下のもの (100℃ or less)[ ]  (2) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)[ ]  (3) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)[ ]  (4) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)[ ]  (5) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)[ ]  (6) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)[ ]  (7) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)[ ]  (8) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)[ ]  (9) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)[ ]  (10) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)[ ]  (11) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)[ ]  (12) 300℃を超えるもの (Exceeding 300℃) |
|  | 二重絶縁 (Double insulation) | [ ]  (1) 施してあるもの (With double insulation)[ ]  (2) 施してないもの (Without double insulation) |