|  | | | **型式の区分** (Type Classification) | | --- | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **特 定 電 気 用 品 名**  (Name of Specified Electrical Appliance and Material) | | **:** | | 冷凍用のショーケース (Freezing showcases) | |
|  | | **要　素** (Factor) | | **区　分** (Classification) | |
|  | | 相 (Phase) | | (1) 単相のもの (Single phase)  (2) ３相のもの (Three phase) | |
|  | | 定格電圧 (Rated voltage) | | (1) 125Ｖ以下のもの (125V or less)  (2) 125Ｖを超えるもの (Exceeding 125V) | |
|  | | 電動機の数 (Number of motor) | | (1) １のもの (One)  (2) ２のもの (Two)  (3) ３以上のもの (Three or more) | |
|  | | 電動機の定格消費電力（圧縮式のものの場合に限る。） (Rated input of electric motor (limited to compressor types.)) | | (1) 50Ｗ以下のもの (50W or less)  (2) 50Ｗを超え60Ｗ以下のもの (Exceeding 50W, and less than or equal to 60W)  (3) 60Ｗを超え70Ｗ以下のもの (Exceeding 60W, and less than or equal to 70W)  (4) 70Ｗを超え80Ｗ以下のもの (Exceeding 70W, and less than or equal to 80W)  (5) 80Ｗを超え90Ｗ以下のもの (Exceeding 80W, and less than or equal to 90W)  (6) 90Ｗを超え100Ｗ以下のもの (Exceeding 90W, and less than or equal to 100W)  (7) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)  (8) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)  (9) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)  (10) 400Ｗを超えるもの (Exceeding 400W) | |
|  | | 電磁振動器の定格消費電力（振動式のものの場合に限る。） (Rated input of electromagnetic oscillator (limited to oscillating types.)) | | (1) 30Ｗ以下のもの (30W or less)  (2) 30Ｗを超え40Ｗ以下のもの (Exceeding 30W, and less than or equal to 40W)  (3) 40Ｗを超え50Ｗ以下のもの (Exceeding 40W, and less than or equal to 50W)  (4) 50Ｗを超え60Ｗ以下のもの (Exceeding 50W, and less than or equal to 60W)  (5) 60Ｗを超え70Ｗ以下のもの (Exceeding 60W, and less than or equal to 70W)  (6) 70Ｗを超え80Ｗ以下のもの (Exceeding 70W, and less than or equal to 80W)  (7) 80Ｗを超え90Ｗ以下のもの (Exceeding 80W, and less than or equal to 90W)  (8) 90Ｗを超え100Ｗ以下のもの (Exceeding 90W, and less than or equal to 100W)  (9) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)  (10) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)  (11) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)  (12) 400Ｗを超えるもの (Exceeding 400W) | |
|  | | 電熱装置 (Heating device) | | (1) あるもの (With heating device)  (2) ないもの (Without heating device) | |
|  | | 電熱装置の定格消費電力 (Rated input of heating device) | | (1) 100Ｗ以下のもの (100W or less)  (2) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)  (3) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)  (4) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)  (5) 400Ｗを超えるもの (Exceeding 400W) | |
|  | | 定格周波数 (Rated frequency) | | (1) 50Hzのもの (50Hz)  (2) 60Hzのもの (60Hz) | |
|  | | 圧縮用電動機 (Compressor motor) | | (1) あるもの (With compressor motor)  (2) ないもの (Without compressor motor) | |
|  | | 圧縮用電動機の種類 (Type of compressor motor) | | (1) 分相始動誘導電動機のもの (Split phase starting induction motor)  (2) コンデンサー始動誘導電動機のもの (Capacity-start induction motor)  (3) コンデンサー誘導電動機のもの (Capacity-run induction motor)  (4) くま取りコイル誘導電動機のもの (Shaded-pole induction motor)  (5) 整流子電動機のもの (Commutator motor)  (6) ３相誘導電動機のもの (Three phase induction motor)  (7) その他のもの (Others) | |
|  | | 圧縮用電動機の極 (Number of compressor motor poles) | | (1) ２極のもの (Two poles)  (2) ４極のもの (Four poles)  (3) ６極のもの (Six poles)  (4) ８極以上のもの (Eight or more poles) | |
|  | | 圧縮用電動機又は電磁振動器の巻線の絶縁の種類 (Compressor motor or electromagnetic oscillator winding insulation class) | | (1) Ａ種のもの (Class A)  (2) Ｅ種のもの (Class E)  (3) Ｂ種のもの (Class B)  (4) Ｆ種のもの (Class F)  (5) Ｈ種のもの (Class H)  (6) その他のもの (Others) | |
|  | | 凝縮器冷却用電動機 (Condenser cooler motor) | | (1) あるもの (With condenser cooler motor)  (2) ないもの (Without condenser cooler motor) | |
|  | | 凝縮器冷却用電動機の種類 (Type of motor condenser cooling) | | (1) 分相始動誘導電動機のもの (Split phase starting induction motor)  (2) コンデンサー始動誘導電動機のもの (Capacity-start induction motor)  (3) コンデンサー誘導電動機のもの (Capacity-run induction motor)  (4) くま取りコイル誘導電動機のもの (Shaded-pole induction motor)  (5) 整流子電動機のもの (Commutator motor)  (6) ３相誘導電動機のもの (Three phase induction motor)  (7) その他のもの (Others) | |
|  | | 凝縮器冷却用電動機の極 (Number of condenser cooling motor poles) | | (1) ２極のもの (Two poles)  (2) ４極のもの (Four poles)  (3) ６極のもの (Six poles)  (4) ８極以上のもの (Eight or more poles) | |
|  | | 凝縮器冷却用電動機の巻線の絶縁の種類 (Condenser cooling motor winding insulation class) | | (1) Ａ種のもの (Class A)  (2) Ｅ種のもの (Class E)  (3) Ｂ種のもの (Class B)  (4) Ｆ種のもの (Class F)  (5) Ｈ種のもの (Class H)  (6) その他のもの (Others) | |
|  | | 器体スイッチ（主回路を開閉するものの場合に限り、自動スイッチ及び自動温度調節器を除く。） (Body switch (limited to those used for turning the main circuit on and off, and excluding temperature limiters and thermostats.)) | | (1) あるもの (With body switch)  (2) ないもの (Without body switch) | |
|  | | 器体スイッチの操作の方式 (Switching operation of body switch) | | (1) タンブラー式のもの (Tumbler type)  (2) 押しボタン式のもの (Push button type)  (3) ロータリー式のもの (Rotary type)  (4) 引きひも式のもの (Pull cord type)  (5) 電磁式のもの (Electromagnetic type)  (6) その他のもの (Others) | |
|  | | 器体スイッチの接点の材料 (Body switch contact materials) | | (1) 銀のもの又は銀合金のもの (Silver or silver alloy)  (2) 銅のもの又は銅合金のもの (Copper or copper alloy)  (3) その他のもの (Others) | |
|  | | 自動温度調節器（温度過昇防止装置として用いられるものを除き、電熱装置から発生する熱により動作するものに限る。） (Thermostat (excluding those used for thermal cutout, and limited to those operating from the heat generated from the electrical heating appliance.)) | | (1) あるもの (With thermostat)  (2) ないもの (Without thermostat) | |
|  | | 温度過昇防止装置 (Thermal cutout) | | (1) あるもの (With thermal cutout)  (2) ないもの (Without thermal cutout) | |
|  | | 温度過昇防止装置の種類 (Type of thermal cutout) | | (1) バイメタル式のもの (Bimetal type)  (2) 温度ヒューズ式のもの (Thermal link type)  (3) その他のもの (Others) | |
|  | | 温度過昇防止装置の動作温度 (Operating temperature of thermal cutout) | | (1) 100℃以下のもの (100℃ or less)  (2) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)  (3) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)  (4) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)  (5) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)  (6) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)  (7) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)  (8) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)  (9) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)  (10) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)  (11) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)  (12) 300℃を超えるもの (Exceeding 300℃) | |
|  | | 冷蔵用のショーケースの冷却媒体 (Refrigerant used in refrigerating showcase) | | (1) 乾式のもの (Dry type)  (2) 湿式のもの (Wet type) | |
|  | | 霜取り用電熱装置 (Defrosting heating device) | | (1) あるもの (With defrosting heating device)  (2) ないもの (Without defrosting heating device) | |
|  | | 露付き防止用電熱装置 (Frost prevention heating device) | | (1) あるもの (With frost prevention heating device)  (2) ないもの (Without frost prevention heating device) | |
|  | | 保温用電熱装置 (Heating device for temperature maintenance) | | (1) あるもの (With heating device for temperature maintenance)  (2) ないもの (Without heating device for temperature maintenance) | |
|  | | 電源電線と器体との接続の方式 (Power supply connections) | | (1) 直付けのもの (Fixed to the appliance)  (2) 接続器利用のもの (Coupling device) | |
|  | | 漏電遮断器 (Residual current operated circuit breakers) | | (1) あるもの (With residual current operated circuit breaker)  (2) ないもの (Without residual current operated circuit breaker) | |
|  | | 二重絶縁 (Double insulation) | | (1) 施してあるもの (With double insulation)  (2) 施してないもの (Without double insulation) | |