|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | 自動販売機 (Vending machines) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 相 (Phase) | [ ]  (1) 単相のもの (Single phase)[ ]  (2) ３相のもの (Three phase) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 定格消費電力（電熱装置の定格消費電力を除く。） (Rated input (excluding the rated input of any electric heating device.)) | [ ]  (1) 40Ｗ以下のもの (40W or less)[ ]  (2) 40Ｗを超え60Ｗ以下のもの (Exceeding 40W, and less than or equal to 60W)[ ]  (3) 60Ｗを超え80Ｗ以下のもの (Exceeding 60W, and less than or equal to 80W)[ ]  (4) 80Ｗを超え100Ｗ以下のもの (Exceeding 80W, and less than or equal to 100W[ ]  (5) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)[ ]  (6) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)[ ]  (7) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)[ ]  (8) 400Ｗを超え500Ｗ以下のもの (Exceeding 400W, and less than or equal to 500W)[ ]  (9) 500Ｗを超え600Ｗ以下のもの (Exceeding 500W, and less than or equal to 600W)[ ]  (10) 600Ｗを超え700Ｗ以下のもの (Exceeding 600W, and less than or equal to 700W)[ ]  (11) 700Ｗを超え800Ｗ以下のもの (Exceeding 700W, and less than or equal to 800W)[ ]  (12) 800Ｗを超え900Ｗ以下のもの (Exceeding 800W, and less than or equal to 900W)[ ]  (13) 900Ｗを超え１kW以下のもの (Exceeding 900W, and less than or equal to 1kW)[ ]  (14) １kWを超え２kW以下のもの (Exceeding 1kW, and less than or equal to 2kW)[ ]  (15) ２kWを超え３kW以下のもの (Exceeding 2kW, and less than or equal to 3kW)[ ]  (16) ３kWを超え５kW以下のもの (Exceeding 3kW, and less than or equal to 5kW)[ ]  (17) ５kWを超えるもの (Exceeding 5kW) |
|  | 定格周波数 (Rated frequency) | [ ]  (1) 50Hzのもの (50Hz)[ ]  (2) 60Hzのもの (60Hz) |
|  | 電動機の数 (Number of motors) | [ ]  (1) １のもの (One)[ ]  (2) ２のもの (Two)[ ]  (3) ３のもの (Three)[ ]  (4) ４のもの (Four)[ ]  (5) ５以上のもの (Five or more) |
|  | 冷却装置 (Cooling device) | [ ]  (1) あるもの (With cooling device)[ ]  (2) ないもの (Without cooling device) |
|  | 冷却の方式 (Cooling method) | [ ]  (1) 圧縮式のもの (Compressor type)[ ]  (2) 振動式のもの (Oscillator type)[ ]  (3) その他のもの (Others) |
|  | 圧縮用電動機の種類 (Type of compressor motor) | [ ]  (1) 分相始動誘導電動機のもの (Split phase starting induction motor)[ ]  (2) コンデンサー始動誘導電動機のもの (Capacity-start induction motor)[ ]  (3) コンデンサー誘導電動機のもの (Capacity-run induction motor)[ ]  (4) くま取りコイル誘導電動機のもの (Shaded-pole induction motor)[ ]  (5) 整流子電動機のもの (Commutator motor)[ ]  (6) ３相誘導電動機のもの (Three phase induction motor)[ ]  (7) その他のもの (Others) |
|  | 圧縮用電動機の極 (Number of compressor motor poles) | [ ]  (1) ２極のもの (Two poles)[ ]  (2) ４極のもの (Four poles)[ ]  (3) ６極のもの (Six poles)[ ]  (4) ８極以上のもの (Eight or more poles) |
|  | 圧縮用電動機又は電磁振動器の巻線の絶縁の種類 (Compressor motor or electromagnetic oscillator winding insulation class) | [ ]  (1) Ａ種のもの (Class A)[ ]  (2) Ｅ種のもの (Class E)[ ]  (3) Ｂ種のもの (Class B)[ ]  (4) Ｆ種のもの (Class F)[ ]  (5) Ｈ種のもの (Class H)[ ]  (6) その他のもの (Others) |
|  | 凝縮器冷却用電動機 (Motor for condenser cooling) | [ ]  (1) あるもの (With motor for condenser cooling)[ ]  (2) ないもの (Without motor for condenser cooling) |
|  | 凝縮器冷却用電動機の種類 (Type of motor condenser cooling) | [ ]  (1) 分相始動誘導電動機のもの (Split phase starting induction motor)[ ]  (2) コンデンサー始動誘導電動機のもの (Capacity-start induction motor)[ ]  (3) コンデンサー誘導電動機のもの (Capacity-run induction motor)[ ]  (4) くま取りコイル誘導電動機のもの (Shaded-pole induction motor)[ ]  (5) 整流子電動機のもの (Commutator motor)[ ]  (6) ３相誘導電動機のもの (Three phase induction motor)[ ]  (7) その他のもの (Others) |
|  | 凝縮器冷却用電動機の極 (Number of condenser cooling motor poles) | [ ]  (1) ２極のもの (Two poles)[ ]  (2) ４極のもの (Four poles)[ ]  (3) ６極のもの (Six poles)[ ]  (4) ８極以上のもの (Eight or more poles) |
|  | 凝縮器冷却用電動機の巻線の絶縁の種類 (Condenser cooling motor winding insulation class) | [ ]  (1) Ａ種のもの (Class A)[ ]  (2) Ｅ種のもの (Class E)[ ]  (3) Ｂ種のもの (Class B)[ ]  (4) Ｆ種のもの (Class F)[ ]  (5) Ｈ種のもの (Class H)[ ]  (6) その他のもの (Others) |
|  | 器体スイッチ（主回路を開閉するものの場合に限り、自動スイッチ及び自動温度調節器を除く。） (Body switch (limited to those used for turning the main circuit on and off, and excluding temperature limiters and thermostats.)) | [ ]  (1) あるもの (With body switch)[ ]  (2) ないもの (Without body switch) |
|  | 器体スイッチの操作の方式 (Switching operation of body switch) | [ ]  (1) タンブラー式のもの (Tumbler type)[ ]  (2) 押しボタン式のもの (Pushbutton type)[ ]  (3) ロータリー式のもの (Rotary type)[ ]  (4) 電磁式のもの (Electromagnetic type)[ ]  (5) その他のもの (Others) |
|  | 器体スイッチの接点の材料 (Body switch contact materials) | [ ]  (1) 銀のもの又は銀合金のもの (Silver or silver alloy)[ ]  (2) 銅のもの又は銅合金のもの (Copper or copper alloy)[ ]  (3) その他のもの (Others) |
|  | 電熱装置 (Electric heating device) | [ ]  (1) あるもの (With heating device)[ ]  (2) ないもの (Without heating device) |
|  | 電熱装置の定格消費電力 (Rated input of electric heating device) | [ ]  (1) 300Ｗ以下のもの (300W or less)[ ]  (2) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)[ ]  (3) 400Ｗを超え500Ｗ以下のもの (Exceeding 400W, and less than or equal to 500W)[ ]  (4) 500Ｗを超え600Ｗ以下のもの (Exceeding 500W, and less than or equal to 600W)[ ]  (5) 600Ｗを超え700Ｗ以下のもの (Exceeding 600W, and less than or equal to 700W)[ ]  (6) 700Ｗを超え800Ｗ以下のもの (Exceeding 700W, and less than or equal to 800W)[ ]  (7) 800Ｗを超え900Ｗ以下のもの (Exceeding 800W, and less than or equal to 900W)[ ]  (8) 900Ｗを超え１kW以下のもの (Exceeding 900W, and less than or equal to 1kW)[ ]  (9) １kWを超え２kW以下のもの (Exceeding 1kW, and less than or equal to 2kW)[ ]  (10) ２kWを超え３kW以下のもの (Exceeding 2kW, and less than or equal to 3kW)[ ]  (11) ３kWを超えるもの (Exceeding 3kW) |
|  | 自動温度調節器（温度過昇防止装置として用いられるものを除き、電熱装置から発生する熱により動作するものに限る。） (Thermostat (excluding those used for thermal cutout, and limited to those operating from the heat generated from the electrical heating appliance.)) | [ ]  (1) あるもの (With thermostat)[ ]  (2) ないもの (Without thermostat) |
|  | 自動温度調節器の温度検知の方式 (Thermostat temperature detection method) | [ ]  (1) バイメタル式のもの (Bimetal type)[ ]  (2) 液体膨張式のもの (Liquid expansion type)[ ]  (3) 気体膨張式のもの (Gas expansion type)[ ]  (4) 半導体式のもの (Semiconductor type)[ ]  (5) その他のもの (Others) |
|  | 自動温度調節器の温度調節の方式 (Thermostat temperature setting method) | [ ]  (1) 接点を機械的に開閉するもの (Mechanical contacts)[ ]  (2) その他のもの (Others) |
|  | 自動温度調節器の動作温度（接点を機械的に開閉するものの場合に限り、かつ、動作温度が可変のものにあつては、その最高温度をいう。） (Thermostat operating temperature (limited to those using mechanical opening and closing of contacts, and, in the case of those with adjustable operating temperature, the maximum temperature.)) | [ ]  (1) 80℃以下のもの (80℃ or less)[ ]  (2) 80℃を超え100℃以下のもの (Exceeding 80℃, and less than or equal to 100℃)[ ]  (3) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)[ ]  (4) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)[ ]  (5) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)[ ]  (6) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)[ ]  (7) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)[ ]  (8) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)[ ]  (9) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)[ ]  (10) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)[ ]  (11) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)[ ]  (12) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)[ ]  (13) 300℃を超えるもの (Exceeding 300℃) |
|  | 用途 (Application) | [ ]  (1) 非包装食品を販売するもの (For selling unpackaged foods)[ ]  (2) その他のもの (Others) |
|  | 霜取り用電熱装置 (Defrosting heating device) | [ ]  (1) あるもの (With defrosting heating device)[ ]  (2) ないもの (Without defrosting heating device) |
|  | 露付き防止用電熱装置 (Frost prevention heating device) | [ ]  (1) あるもの (With frost prevention heating device)[ ]  (2) ないもの (Without frost prevention heating device) |
|  | 保温用電熱装置 (Electric heating device for temperature maintenance) | [ ]  (1) あるもの (With heating device for temperature maintenance)[ ]  (2) ないもの (Without heating device for temperature maintenance) |
|  | 発振管 (Oscillating tube) | [ ]  (1) あるもの (With oscillating tube)[ ]  (2) ないもの (Without oscillating tube) |
|  | 放電灯 (Discharge lamp) | [ ]  (1) あるもの (With discharge lamp)[ ]  (2) ないもの (Without discharge lamp) |
|  | 液体収納装置 (Liquid storage compartment) | [ ]  (1) あるもの (With liquid storage compartment)[ ]  (2) ないもの (Without liquid storage compartment) |
|  | 使用場所 (Place for use) | [ ]  (1) 屋外のもの (Outdoors)[ ]  (2) 屋内のもの (Indoors) |
|  | 電源電線と器体との接続の方式 (Power supply connections) | [ ]  (1) 直付けのもの (Fixed to the appliance)[ ]  (2) 接続器利用のもの (Coupling device) |
|  | 温度過昇防止装置 (Thermal cutout) | [ ]  (1) あるもの (With thermal cutout)[ ]  (2) ないもの (Without thermal cutout) |
|  | 温度過昇防止装置の種類 (Type of thermal cutout) | [ ]  (1) バイメタル式のもの (Bimetal type)[ ]  (2) 温度ヒューズ式のもの (Thermal link type)[ ]  (3) その他のもの (Others) |
|  | 温度過昇防止装置の動作温度 (Operating temperature of thermal cutout) | [ ]  (1) 100℃以下のもの (100℃ or less)[ ]  (2) 100℃を超え120℃以下のもの (Exceeding 100℃, and less than or equal to 120℃)[ ]  (3) 120℃を超え140℃以下のもの (Exceeding 120℃, and less than or equal to 140℃)[ ]  (4) 140℃を超え160℃以下のもの (Exceeding 140℃, and less than or equal to 160℃)[ ]  (5) 160℃を超え180℃以下のもの (Exceeding 160℃, and less than or equal to 180℃)[ ]  (6) 180℃を超え200℃以下のもの (Exceeding 180℃, and less than or equal to 200℃)[ ]  (7) 200℃を超え220℃以下のもの (Exceeding 200℃, and less than or equal to 220℃)[ ]  (8) 220℃を超え240℃以下のもの (Exceeding 220℃, and less than or equal to 240℃)[ ]  (9) 240℃を超え260℃以下のもの (Exceeding 240℃, and less than or equal to 260℃)[ ]  (10) 260℃を超え280℃以下のもの (Exceeding 260℃, and less than or equal to 280℃)[ ]  (11) 280℃を超え300℃以下のもの (Exceeding 280℃, and less than or equal to 300℃)[ ]  (12) 300℃を超えるもの (Exceeding 300℃) |
|  | 漏電遮断器 (Residual current operated circuit breakers) | [ ]  (1) あるもの (With residual current operated circuit breakers)[ ]  (2) ないもの (Without residual current operated circuit breakers) |
|  | 二重絶縁 (Double insulation) | [ ]  (1) 施してあるもの (With double insulation)[ ]  (2) 施してないもの (Without double insulation) |