|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | 携帯発電機 (Portable power generators) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 相 (Phase) | [ ]  (1) 単相のもの (Single phase)[ ]  (2) ３相のもの (Three phase) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 定格出力（交流のものの場合に限る。） (Rated output (limited to alternating current type.)) | [ ]  (1) 100VA以下のもの (100VA or less)[ ]  (2) 100VAを超え200VA以下のもの (Exceeding 100VA, and less than or equal to 200VA)[ ]  (3) 200VAを超え300VA以下のもの (Exceeding 200VA, and less than or equal to 300VA)[ ]  (4) 300VAを超え400VA以下のもの (Exceeding 300VA, and less than or equal to 400VA)[ ]  (5) 400VAを超え500VA以下のもの (Exceeding 400VA, and less than or equal to 500VA)[ ]  (6) 500VAを超え600VA以下のもの (Exceeding 500VA, and less than or equal to 600VA)[ ]  (7) 600VAを超え700VA以下のもの (Exceeding 600VA, and less than or equal to 700VA)[ ]  (8) 700VAを超え800VA以下のもの (Exceeding 700VA, and less than or equal to 800VA)[ ]  (9) 800VAを超え900VA以下のもの (Exceeding 800VA, and less than or equal to 900VA)[ ]  (10) 900VAを超え１kVA以下のもの (Exceeding 900VA, and less than or equal to 1kVA)[ ]  (11) １kVAを超え２kVA以下のもの (Exceeding 1kVA, and less than or equal to 2kVA)[ ]  (12) ２kVAを超えるもの (Exceeding 2kVA) |
|  | 定格出力（直流のものの場合に限る。） (Rated output (limited to direct current type.)) | [ ]  (1) 100Ｗ以下のもの (100W or less)[ ]  (2) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)[ ]  (3) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)[ ]  (4) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)[ ]  (5) 400Ｗを超え500Ｗ以下のもの (Exceeding 400W, and less than or equal to 500W)[ ]  (6) 500Ｗを超え600Ｗ以下のもの (Exceeding 500W, and less than or equal to 600W)[ ]  (7) 600Ｗを超え700Ｗ以下のもの (Exceeding 600W, and less than or equal to 700W)[ ]  (8) 700Ｗを超え800Ｗ以下のもの (Exceeding 700W, and less than or equal to 800W)[ ]  (9) 800Ｗを超え900Ｗ以下のもの (Exceeding 800W, and less than or equal to 900W)[ ]  (10) 900Ｗを超え１kW以下のもの (Exceeding 900W, and less than or equal to 1kW)[ ]  (11) １kWを超え２kW以下のもの (Exceeding 1kW, and less than or equal to 2kW)[ ]  (12) ２kWを超えるもの (Exceeding 2kW) |
|  | 発電機の種類 (Type of generator) | [ ]  (1) 交流発電機のもの (Alternating current generator)[ ]  (2) 直流発電機のもの (Direct current generator) |
|  | 出力の種類 (Type of output) | [ ]  (1) 交流のもの (A.C. output)[ ]  (2) 直流のもの (D.C. output) |
|  | 定格出力周波数（出力の種類が交流のものの場合に限る。） (Rated output frequency (limited to those with alternating current output.)) | [ ]  (1) 50Hzのもの (50 Hz)[ ]  (2) 60Hzのもの (60 Hz)[ ]  (3) その他のもの (Others) |
|  | 巻線の絶縁の種類 (Winding insulation class) | [ ]  (1) Ａ種のもの (Class A)[ ]  (2) Ｅ種のもの (Class E)[ ]  (3) Ｂ種のもの (Class B)[ ]  (4) Ｆ種のもの (Class F)[ ]  (5) Ｈ種のもの (Class H)[ ]  (6) その他のもの (Others) |
|  | 原動機の種類 (Type of engine) | [ ]  (1) 火花点火機関のもの (Spark ignition type)[ ]  (2) 圧縮点火機関のもの (Compression ignition type)[ ]  (3) その他のもの (Others) |