|  | | | **型式の区分** (Type Classification) | | --- | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **特 定 電 気 用 品 名**  (Name of Specified Electrical Appliance and Material) | | **:** | | ミシン用コントローラー (Sewing machine controllers) | |
|  | | **要　素** (Factor) | | **区　分** (Classification) | |
|  | | 定格電圧 (Rated voltage) | | (1) 125Ｖ以下のもの (125V or less)  (2) 125Ｖを超えるもの (Exceeding 125V) | |
|  | | 適用電動機の入力（定格出力が50Ｗ以下のものの場合に限る。） (Input power of applicable motor (limited to those with rated output of 50W or less.)) | | (1) 30Ｗ以下のもの (30W or less)  (2) 30Ｗを超え35Ｗ以下のもの (Exceeding 30W, and less than or equal to 35W)  (3) 35Ｗを超え40Ｗ以下のもの (Exceeding 35W, and less than or equal to 40W)  (4) 40Ｗを超え45Ｗ以下のもの (Exceeding 40W, and less than or equal to 45W)  (5) 45Ｗを超え50Ｗ以下のもの (Exceeding 45W, and less than or equal to 50W)  (6) 50Ｗを超え55Ｗ以下のもの (Exceeding 50W, and less than or equal to 55W)  (7) 55Ｗを超え60Ｗ以下のもの (Exceeding 55W, and less than or equal to 60W)  (8) 60Ｗを超え65Ｗ以下のもの (Exceeding 60W, and less than or equal to 65W)  (9) 65Ｗを超え70Ｗ以下のもの (Exceeding 65W, and less than or equal to 70W)  (10) 70Ｗを超え75Ｗ以下のもの (Exceeding 70W, and less than or equal to 75W)  (11) 75Ｗを超え80Ｗ以下のもの (Exceeding 75W, and less than or equal to 80W)  (12) 80Ｗを超えるもの (Exceeding 80W) | |
|  | | 適用電動機の出力（定格出力が50Ｗを超えるものの場合に限る。） (Output power of applicable motor (limited to those with rated output of exceeding 50W.)) | | (1) 50Ｗを超え60Ｗ以下のもの (Exceeding 50W, and less than or equal to 60W)  (2) 60Ｗを超え80Ｗ以下のもの (Exceeding 60W, and less than or equal to 80W)  (3) 80Ｗを超え100Ｗ以下のもの (Exceeding 80W, and less than or equal to 100W)  (4) 100Ｗを超え125Ｗ以下のもの (Exceeding 100W, and less than or equal to 125W)  (5) 125Ｗを超え150Ｗ以下のもの (Exceeding 125W, and less than or equal to 150W)  (6) 150Ｗを超え200Ｗ以下のもの (Exceeding 150W, and less than or equal to 200W)  (7) 200Ｗを超え250Ｗ以下のもの (Exceeding 200W, and less than or equal to 250W)  (8) 250Ｗを超え350Ｗ以下のもの (Exceeding 250W, and less than or equal to 350W)  (9) 350Ｗを超え450Ｗ以下のもの (Exceeding 350W, and less than or equal to 450W)  (10) 450Ｗを超え550Ｗ以下のもの (Exceeding 450W, and less than or equal to 550W)  (11) 550Ｗを超え650Ｗ以下のもの (Exceeding 550W, and less than or equal to 650W)  (12) 650Ｗを超え750Ｗ以下のもの (Exceeding 650W, and less than or equal to 750W)  (13) 750Ｗを超えるもの (Exceeding 750W) | |
|  | | 制御の方式 (Control method) | | (1) 半導体利用のもの (Semiconductor control)  (2) その他のもの (Others) | |
|  | | 抵抗値の変更の方式（半導体利用のものの場合を除く。） (Method of changing resistance value (excluding those using　semiconductors.)) | | (1) 炭素パイル式のもの (Carbon pile type)  (2) 摺動式のもの (Sliding type)  (3) タップ式のもの (Tap type)  (4) その他のもの (Others) | |
|  | | 主絶縁体の材料 (Insulation materials) | | (1) 磁器のもの (Ceramic)  (2) 合成樹脂のもの (Plastic)  (3) その他のもの (Others) | |
|  | | 外郭の材料 (Outer case materials) | | (1) 金属のもの (Metal)  (2) 合成樹脂のもの (Plastic)  (3) その他のもの (Others) | |