|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | ミシン用コントローラー (Sewing machine controllers) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) 125Ｖ以下のもの (125V or less)[ ]  (2) 125Ｖを超えるもの (Exceeding 125V) |
|  | 適用電動機の入力（定格出力が50Ｗ以下のものの場合に限る。） (Input power of applicable motor (limited to those with rated output of 50W or less.)) | [ ]  (1) 30Ｗ以下のもの (30W or less)[ ]  (2) 30Ｗを超え35Ｗ以下のもの (Exceeding 30W, and less than or equal to 35W)[ ]  (3) 35Ｗを超え40Ｗ以下のもの (Exceeding 35W, and less than or equal to 40W)[ ]  (4) 40Ｗを超え45Ｗ以下のもの (Exceeding 40W, and less than or equal to 45W)[ ]  (5) 45Ｗを超え50Ｗ以下のもの (Exceeding 45W, and less than or equal to 50W)[ ]  (6) 50Ｗを超え55Ｗ以下のもの (Exceeding 50W, and less than or equal to 55W)[ ]  (7) 55Ｗを超え60Ｗ以下のもの (Exceeding 55W, and less than or equal to 60W)[ ]  (8) 60Ｗを超え65Ｗ以下のもの (Exceeding 60W, and less than or equal to 65W)[ ]  (9) 65Ｗを超え70Ｗ以下のもの (Exceeding 65W, and less than or equal to 70W)[ ]  (10) 70Ｗを超え75Ｗ以下のもの (Exceeding 70W, and less than or equal to 75W)[ ]  (11) 75Ｗを超え80Ｗ以下のもの (Exceeding 75W, and less than or equal to 80W)[ ]  (12) 80Ｗを超えるもの (Exceeding 80W) |
|  | 適用電動機の出力（定格出力が50Ｗを超えるものの場合に限る。） (Output power of applicable motor (limited to those with rated output of exceeding 50W.)) | [ ]  (1) 50Ｗを超え60Ｗ以下のもの (Exceeding 50W, and less than or equal to 60W)[ ]  (2) 60Ｗを超え80Ｗ以下のもの (Exceeding 60W, and less than or equal to 80W)[ ]  (3) 80Ｗを超え100Ｗ以下のもの (Exceeding 80W, and less than or equal to 100W)[ ]  (4) 100Ｗを超え125Ｗ以下のもの (Exceeding 100W, and less than or equal to 125W)[ ]  (5) 125Ｗを超え150Ｗ以下のもの (Exceeding 125W, and less than or equal to 150W)[ ]  (6) 150Ｗを超え200Ｗ以下のもの (Exceeding 150W, and less than or equal to 200W)[ ]  (7) 200Ｗを超え250Ｗ以下のもの (Exceeding 200W, and less than or equal to 250W)[ ]  (8) 250Ｗを超え350Ｗ以下のもの (Exceeding 250W, and less than or equal to 350W)[ ]  (9) 350Ｗを超え450Ｗ以下のもの (Exceeding 350W, and less than or equal to 450W)[ ]  (10) 450Ｗを超え550Ｗ以下のもの (Exceeding 450W, and less than or equal to 550W)[ ]  (11) 550Ｗを超え650Ｗ以下のもの (Exceeding 550W, and less than or equal to 650W)[ ]  (12) 650Ｗを超え750Ｗ以下のもの (Exceeding 650W, and less than or equal to 750W)[ ]  (13) 750Ｗを超えるもの (Exceeding 750W) |
|  | 制御の方式 (Control method) | [ ]  (1) 半導体利用のもの (Semiconductor control)[ ]  (2) その他のもの (Others) |
|  | 抵抗値の変更の方式（半導体利用のものの場合を除く。） (Method of changing resistance value (excluding those using　semiconductors.)) | [ ]  (1) 炭素パイル式のもの (Carbon pile type)[ ]  (2) 摺動式のもの (Sliding type)[ ]  (3) タップ式のもの (Tap type)[ ]  (4) その他のもの (Others) |
|  | 主絶縁体の材料 (Insulation materials) | [ ]  (1) 磁器のもの (Ceramic)[ ]  (2) 合成樹脂のもの (Plastic)[ ]  (3) その他のもの (Others) |
|  | 外郭の材料 (Outer case materials) | [ ]  (1) 金属のもの (Metal)[ ]  (2) 合成樹脂のもの (Plastic)[ ]  (3) その他のもの (Others) |