|  |

| **型式の区分** (Type Classification) |
| --- |

 |
| --- | --- | --- |
|  | **特 定 電 気 用 品 名**(Name of Specified Electrical Appliance and Material) | **:** | アダプター (Adaptors) |
|  | **要　素** (Factor) | **区　分** (Classification) |
|  | 定格電圧 (Rated voltage) | [ ]  (1) １２５Ｖ以下のもの (125V or less)[ ]  (2) １２５Ｖを超えるもの (Exceeding 125V) |
|  | 定格電流 (Rated current) | [ ]  (1) １Ａ以下のもの (1A or less)[ ]  (2) １Ａを超え３Ａ以下のもの (Exceeding 1A, and less than or equal to 3A)[ ]  (3) ３Ａを超え７Ａ以下のもの (Exceeding 3A, and less than or equal to 7A)[ ]  (4) ７Ａを超え１０Ａ以下のもの (Exceeding 7A, and less than or equal to 10A)[ ]  (5) １０Ａを超えるもの (Exceeding 10A) |
|  | 電源側の接続部の形状 (Shape of connector on power supply side) | [ ]  (1) 刃型（ピン型を含む。）のもの (Blade shape (including pin types.)[ ]  (2) ねじ込み型（スワン型を含む。）のもの (Screw in type (including swan types.)[ ]  (3) その他のもの (Others) |
|  | 負荷側の接続部の形状 (Shape of connector on load side) | [ ]  (1) 刃型（ピン型を含む。）のもの (Blade shape (including pin types.))[ ]  (2) ねじ込み型（スワン型を含む。）のもの (Screw in type (including swan types.))[ ]  (3) その他のもの (Others) |
|  | 主絶縁体の材料 (Insulation materials) | [ ]  (1) 合成樹脂のもの (Plastic)[ ]  (2) その他のもの (Others) |
|  | スイッチ (Switch) | [ ]  (1) あるもの (With switch)[ ]  (2) ないもの (Without switch) |
|  | 中間口出し線（中間口出し線用端子を含む。） (Intermediate lead wire (including intermediate lead wire terminal.)) | [ ]  (1) あるもの (With intermediate lead wire)[ ]  (2) ないもの (Without intermediate lead wire) |