|  | | | **型式の区分** (Type Classification) | | --- | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | **特 定 電 気 用 品 名**  (Name of Specified Electrical Appliance and Material) | | **:** | | 携帯発電機 (Portable power generators) | |
|  | | **要　素** (Factor) | | **区　分** (Classification) | |
|  | | 相 (Phase) | | (1) 単相のもの (Single phase)  (2) ３相のもの (Three phase) | |
|  | | 定格電圧 (Rated voltage) | | (1) 125Ｖ以下のもの (125V or less)  (2) 125Ｖを超えるもの (Exceeding 125V) | |
|  | | 定格出力（交流のものの場合に限る。） (Rated output (limited to alternating current type.)) | | (1) 100VA以下のもの (100VA or less)  (2) 100VAを超え200VA以下のもの (Exceeding 100VA, and less than or equal to 200VA)  (3) 200VAを超え300VA以下のもの (Exceeding 200VA, and less than or equal to 300VA)  (4) 300VAを超え400VA以下のもの (Exceeding 300VA, and less than or equal to 400VA)  (5) 400VAを超え500VA以下のもの (Exceeding 400VA, and less than or equal to 500VA)  (6) 500VAを超え600VA以下のもの (Exceeding 500VA, and less than or equal to 600VA)  (7) 600VAを超え700VA以下のもの (Exceeding 600VA, and less than or equal to 700VA)  (8) 700VAを超え800VA以下のもの (Exceeding 700VA, and less than or equal to 800VA)  (9) 800VAを超え900VA以下のもの (Exceeding 800VA, and less than or equal to 900VA)  (10) 900VAを超え１kVA以下のもの (Exceeding 900VA, and less than or equal to 1kVA)  (11) １kVAを超え２kVA以下のもの (Exceeding 1kVA, and less than or equal to 2kVA)  (12) ２kVAを超えるもの (Exceeding 2kVA) | |
|  | | 定格出力（直流のものの場合に限る。） (Rated output (limited to direct current type.)) | | (1) 100Ｗ以下のもの (100W or less)  (2) 100Ｗを超え200Ｗ以下のもの (Exceeding 100W, and less than or equal to 200W)  (3) 200Ｗを超え300Ｗ以下のもの (Exceeding 200W, and less than or equal to 300W)  (4) 300Ｗを超え400Ｗ以下のもの (Exceeding 300W, and less than or equal to 400W)  (5) 400Ｗを超え500Ｗ以下のもの (Exceeding 400W, and less than or equal to 500W)  (6) 500Ｗを超え600Ｗ以下のもの (Exceeding 500W, and less than or equal to 600W)  (7) 600Ｗを超え700Ｗ以下のもの (Exceeding 600W, and less than or equal to 700W)  (8) 700Ｗを超え800Ｗ以下のもの (Exceeding 700W, and less than or equal to 800W)  (9) 800Ｗを超え900Ｗ以下のもの (Exceeding 800W, and less than or equal to 900W)  (10) 900Ｗを超え１kW以下のもの (Exceeding 900W, and less than or equal to 1kW)  (11) １kWを超え２kW以下のもの (Exceeding 1kW, and less than or equal to 2kW)  (12) ２kWを超えるもの (Exceeding 2kW) | |
|  | | 発電機の種類 (Type of generator) | | (1) 交流発電機のもの (Alternating current generator)  (2) 直流発電機のもの (Direct current generator) | |
|  | | 出力の種類 (Type of output) | | (1) 交流のもの (A.C. output)  (2) 直流のもの (D.C. output) | |
|  | | 定格出力周波数（出力の種類が交流のものの場合に限る。） (Rated output frequency (limited to those with alternating current output.)) | | (1) 50Hzのもの (50 Hz)  (2) 60Hzのもの (60 Hz)  (3) その他のもの (Others) | |
|  | | 巻線の絶縁の種類 (Winding insulation class) | | (1) Ａ種のもの (Class A)  (2) Ｅ種のもの (Class E)  (3) Ｂ種のもの (Class B)  (4) Ｆ種のもの (Class F)  (5) Ｈ種のもの (Class H)  (6) その他のもの (Others) | |
|  | | 原動機の種類 (Type of engine) | | (1) 火花点火機関のもの (Spark ignition type)  (2) 圧縮点火機関のもの (Compression ignition type)  (3) その他のもの (Others) | |